INFIE10:IEAJ011.EPS

PSL2-Program code: raster cell-threshold data (24 × 24, 8 bit, horizontal)