AEB80-3N

VG -> VG Original VG with standard gamma gP=1,000

File graphic ISO step gamma g_P AEB80-1N VG C_{YP8}=C_{YN8} 1,000 Application: luminance contrast of sRGB displays: Y_W : Y_N = 90 : 0,31 = 288 : 1 according to ISO 9241-306. (contrast without display reflection of room light)