AEB80-8N

VG -> PG

Change original VG with gamma gP=0,850

File graphic ISO step gamma g_P AEB80-7N PG C_{YP6}=C_{YN10} 0,850 Application: mean luminance contrast of displays: Y_W : Y_N = 90 : 1,25 = 72 : 1 according to ISO 9241-306. (contrast higher offset paper according to ISO/IEC 15775)