AEG30-2N,13

Colorimetric filter transfer i = 1 c*_1 = a c*n with a = 1,00; n = 1,00 rgb -> rgb* rgb* -> rgb*_1