BET50-7N

Basic television colour or mixture colour for D65 CIE data for YW=100 chromaticity

xd yd tristimulus values

(Yd=100,0 for white D65)

Xd Yd Zd

three additive mixture colours of ITU-R BT.2020-2,WCGa, Wide Colour Gamut Cd Md Yd Cyan (Cyan blue) Magenta (magenta red) Yellow

0,146 0,368 0,446

0,344 0,147 0,537

31,34 80,58 78,15

73,72 32,20 94,07

108,90 106,09 2,80

three additive basic colours of ITU-R BT.2020-2, WCGa, Wide Colour Gamut Rd Gd Bd Red (orange red) Green (leaf green) Blue (violet blue)

0,708 0,170 0,131

0,292 0,797 0,046

63,69 14,46 16,88

26,27 67,80 5,93

0,00 2,80 106,09

achromatic colours with different normalization:

W0 (white monitor, 100%) W1 (white monitor, 88,6%) N1 (black monitor, 2,5%) N0 (black monitor, 0,00%)

0,312 0,329 95,05 100,00 108,90 0,312 0,329 84,21 88,60 96,48 0,312 0,329 2,37 2,50 2,72 0,312 0,329 0,00 0,00 0,00