BET61-3N

Basic television colour or mixture colour for D65 CIE data for YW=88,6

three additive mixture colours of ITU-R BT.709.3, sRGB, IEC 61966-2-1 Cd Md Yd Cyan (Cyan blue) Magenta (magenta red) Yellow

86,88 57,30 92,66

-46,18 94,34 -20,72

-13,57 -58,43 90,74

48,13 110,97 93,08 199 324 110

Standard CIELAB data L*a*b*C*abhab

(L*d=88,6 for white; L*d=18,0 for black)

L*d a*d b*d C*ab,d hab,d

three additive basic colours of ITU-R BT.709.3, sRGB, IEC 61966-2-1 Rd Gd Bd Red (orange red) Green (leaf green) Blue (violet blue)

50,49 83,63 30,39

76,91 -82,78 76,06

64,54 79,89 -103,59

100,40 115,04 128,52 19 144 290 achromatic colours with different normalization:

W0 (white monitor, 100%) W1 (white monitor, 88,6%) N1 (black monitor, 2,5%) N0 (black monitor, 0,00%)

100,00 0,00 0,00 0,00 0 95,40 0,00 0,00 0,00 0 18,00 0,00 0,00 0,00 0 0,00 0,00 0,00 0,00 0