BET70-3N

Basic television colour or mixture colour for D65 CIE data for YW=100

three additive mixture colours of ITU-R BT.709.3, sRGB, IEC 61966-2-1 Cd Md Yd Cyan (Cyan blue) Magenta (magenta red) Yellow

78,73 28,48 92,78

-52,62 53,52 -0,92

-16,98 -52,78 69,75

55,30 75,17 69,75 197 315 90

Standard dataYA2B2CAB2hAB2

(Yd=100,0 for white; Yd=0,0 for black)

Yd A2d B2d CAB2,d hAB2,d

three additive basic colours of ITU-R BT.709.3, sRGB, IEC 61966-2-1 Rd Gd Bd Red (orange red) Green (leaf green) Blue (violet blue)

21,26 71,52 7,22

52,61 -53,54 0,91

16,97 52,77 -69,76

55,28 75,17 69,76 17 135 270 achromatic colours with different normalization:

C_{AB2,d} = [A_{2d}^2 + B_{2d}^2]^{1/2}; h_{AB2,d} = atan[B_{2d} / A_{2d}] compare CIE 230:2019

W0 (white monitor, 100%) W1 (white monitor, 88,6%) N1 (black monitor, 2,5%) N0 (black monitor, 0,00%)

100,00 0,00 0,00 0,00 0 88,60 0,00 0,00 0,00 0 2,50 0,00 0,00 0,00 0 0,00 0,00 0,00 0,00 0