DEB50-4A

x_r = log[ L/L_u]

L_u L_u=28cd/m^2

range of office luminance

Q_{ab}(x_r)=achromatic receptor response & modified

W

N