OE801-3N-030-2: File: Measure unknown; Device: Device unknown; Date: Date unknown

N 0,0 0,25 0,50 0,75 1,00 W

N 0,00

0,25

0,50

0,75

W 1,00 w*’output w’*output

w*input

For linearized output of the 16 grey steps of Picture A7-030-2 ’* (dash-star) coordinates to reach the linearized output with the real display reflection in office room; lighter (positiv P) output w’*_{output} = [w*_{input}] 1.00

*’ (star-dash) coordinates of real output with real display reflection in office room; darker (negativ N) output w*’_{output} = [w*_{input}] 1.00