Part 4 OE871-7N-030-1

Documentation of assessor colour vision properties for visual assessment

The assessor has normal colour vision according to one test: underline Yes/No either according to DIN 6160:1996 with Anomaloskop of Nagel underline Yes/unknown or with test charts using colour points according to Ishihara underline Yes/unknown or tested with, please specify: ................................... underline Yes/unknown

For visual evaluation of the display (monitor, data projector) output

Office workplace illumination is daylight (clouded/north sky) underline Yes/No PDF file: http://130.149.60.45/farbmetrik/OE87/OE87F1P2.PDF underline Yes/No PS file: http://130.149.60.45/farbmetrik/OE87/OE87F1P2.PS underline Yes/No Picture A7-030-2: contrast range: (>F:0) (F:0) (E:0) (D:0) (C:0) (A:0) (9:0) (7:0) (5:0) (3:0) (<3:0) compare standard print output according to ISO/IEC 15775 with range F:0 underline range Remark: In daylighted offices the contrast range is in many cases: on display between: >F:0 and E:0 (monitor), D:0 and 3:0 (data projector)

Only for optional colorimetric specification with PDF/PS file output

PDF-File: http://130.149.60.45/farbmetrik/OE87/OE87F1P2.PDF picture A7-030-2 underline Yes/No PS-File: http://130.149.60.45/farbmetrik/OE87/OE87F1P2.PS picture A7-030-2 or underline Yes/No colour measurement and specification for:

CIE standard illuminant D65, 2 degree observer, CIE 45/0 geometry: underline Yes/No If No, please give other parameters: ...........................................

Colorimetric specification with PS file for colours in the columns A to T

Exchange of CIELAB data in file www.ps.bam.de/De17/10L/L17e00NP.PS and transfer of the PS-file L17e00NP.PS in PDF-file L17e00NP.PDF underline Yes/No If No, please describe other method: ......................................