heb31-7a, eer30-5n

IECsRGB lightness logT*_u as function of logY coordinates logT*_u and logY for achromatic colours

logY Y logT*_u T*_u

48,9T*_u

Y_u=18 m=1/2,4

3,6, 3,618, 3,690, 3,6Y, T*_u

IECsRGB lightness: T*_u = 48,9 (Y/Y_u)^{1/2,4} (Y_u=18, Y>0,1) applicationrange