YE960-3

Colorimetric data of six chromatic basic colours X = OYLCVM of a device system

colorimetric name family family member coordinate kind coordinate (compare CIELAB L*, C*_{ab}, h_{ab}, a*, b*) coordinate name

standard CIELAB

adapted CIELAB (a)

relative CIELAB (r)

LAB*

LAB*_a

lab*

LAB*LCH*_X or LAB*LAB*_X

LAB*_aLCH*_{a,X} or LAB*_aLAB*_{a,X}

lab*lch*_X or lab*lab*_X zylindric or kartesic

zylindric or kartesic

zylindric or kartesic

L*_X = LAB*L*_X C*_X = LAB*C*_{ab,M} H*_X = LAB*h_{ab,M} A*_X = LAB*a*_X B*_X = LAB*b*_X

L*_{a,X} = LAB*_aL*_{a,X} C*_{a,X} = LAB*_aC*_{a,X} H*_{a,X} = LAB*_aH*_{a,X}

l*_X = lab*l*_X c*_X = lab*c*_X h*_X = lab*h*_X lightness chroma hue angle red green chroma yellow blue chroma

adapted lightness ( = L*_X) adapted chroma adapted hue angle ( 0 <= H*_{a,X} <= 360 )

relative lightness relative chroma relative hue ( 0,00 <= h*_X <= 1,00 )