Part 3 LE951-3, De150-3

Agreement with elementary hues (Yes/No decision) HP Laserjet CP1514n

There are four elementary hues on each page: Red R, Yellow J (=french Jaune), Green G, and Blue B. Input data 1 0 0 should produce Red R. Input data 0 1 0 should produce Green G. Input data 0 0 1 should produce Blue B. Input data 1 1 0 should produce Yellow J. The elementary hues Red R and Green G should locate on the horizontal axis. The elementary hues Yellow J and Blue B should locate on the vertical axis. This test uses a hue circle with 20 hues.

No. 00 and 10 should be Red R and Green G. No. 05 and 15 should be Yellow J and Blue B.

Are no. 00, 05, 10, and 15 the four elementary hues R, J, G and B? underline: Yes/No Only in case of "No":

Elementary Red R is hue step no. (e. g. 00, 01, 19) ........

00 (neither yellowish nor blueish) Elementary Yellow J is hue step no. (e. g. 05, 04, 06) ........

05 (neither reddish nor greenish) Elementary Green G is hue step no. (e. g. 10, 09, 11) ........

10 (neither yellowish nor blueish) Elementary Blue B is hue step no. (e. g. 15, 14, 16) ........

14 (neither reddish nor greenish) Result: Of the 4 elementary hues (e.g. three) .........

3 are at the intended location

Layout example: agreement with elementary hues Test chart 2 according to DIN 33872-5

= R?